Section A, Rev. 1, 11/20/03
Apartment Entry Systems— CM193 & CM493—with handset remote and door release, 28+ units


Engineers’ Specification

1.0 General

A.
The contractor shall provide and install all equipment, accessories and materials necessary for a complete operating system in accordance with the following specifications.

B.
The equipment furnished under this specification shall be the standard product of one manufacturer and shall be as manufactured by TekTone Sound & Signal Mfg., Inc.

C.
The contractor shall guarantee availability of local service and available stock of the manufacturers standard parts.

D.
The contractor shall be responsible for providing a complete functional system including all necessary components, whether included in this specification or not.

1.1 Systems Operation

The apartment entry system shall operate as follows:

A.
The visitor, by depressing the appropriate room call button on the entry panel, shall sound a tone to the handset remote in the apartment or office.

B.
The tenant or office, by picking up the phone, shall carry on two-way communication with the visitor. Talk/Listen button(s) shall be unacceptable.

C.
After acknowledging the visitor, the tenant shall press the door release button on the handset releasing the entrance door into the building.

1.2 Function Options

A.
Multiple entrances

B.
Postal Release

2.0 EQUIPMENT

2.1 Apartment

The suite station shall be a TA205B handset and have:

A.
Dynamic speaker/microphone.

B.
Duplex communication. The use of talk/listen button(s) shall not be acceptable. 

C.
Plug in handset.

D.
Door release button in handset.

E.
Be constructed of ABS plastic with mechanical hook switch.

F.
Mount on single gang ring or box.

2.2 Entrance Panel: 

The entrance panel shall be CM193/xx or CM493/xx (vandal) and have:

A.
Extruded aluminum construction

B.
One (1) self-wiping button for each apartment.

C.
One (1) 2.5" Mylar speaker

D.
One (1) 1.75" Mylar speaker (mic)

2.2.1
Panel Options

A.
Expansion panels shall be added using CM190/xx for standard panels and CM490/xx for vandal panels.

B.
Panel mounting shall be OF190 series frame and OH190 series box. Surface mounting shall be OF190S series surface frame.

C.
For multiple entrances, use one PK502B relay per additional entrance.

D.
For postal release option, add the suffix “P” to the panel model number. (Note: addition of postal reduces that panel button capacity by eight (8).

2.2.2 Directory Panel

The directory panel(s) shall be AM190D and have:

A.
Extruded aluminum construction

B.
Lexan window

C.
Accommodations for 60 names

2.3 Amplifier

The amplifier/power pack shall be PK205 and have:

A.
Separate controls for audio and call tone volume accessible from the front of the panel.

B.
Screw terminals for wire terminations

C.
Rugged extruded aluminum housing

2.4 Door Strike

The door strike shall be PO001 for standard duty mortise type installation, and operate on 16VAC.

2.5 Transformer

The transformer shall be SS102A (hard-wire) or SS105B (plug-in), 16VAC, 10VA and be UL listed.

Part 3—Wiring
System wiring shall be five (5) wires consisting of four (4) common conductors and one (1) selective conductor for each suite. Wiring shall be in strict accord with TekTone IL418 wiring diagram (and IL 499 when using the PK502B dual entrance relay.)

Part 4—Warranty
Each piece of equipment shall be warranted by the equipment manufacturer to be free of defects in material and workmanship for a period of twelve (12) months from the date of shipment from the factory.

Part 5—Shop Drawings
The electrical contractor shall submit shop drawings to the electrical engineer for approval. The contractor must have approved shop drawings in his possession prior to installation.
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